Standard Performance Evaluation Corporation info@spec.org http://www.spec.org/

Page 1 spec^® SPEC

® CINT2006 Result

Copyright 2006-2014 Standard Performance Evaluation Corporation

Sun Microsystems Sun SPARC Enterprise M3000

SPECint^®_rate2006 = 40.8

SPECint_rate_base2006 = 36.9

CPU2006 license: 6 Test date: Sep-2008 Test sponsor: Sun Microsystems Hardware Availability: Oct-2008 Tested by: Fujitsu Limited Software Availability: Oct-2008

400.perlbench

401.bzip2

403.gcc

429.mcf

445.gobmk

456.hmmer

458.sjeng

462.libquantum

464.h264ref

471.omnetpp

473.astar

483.xalancbmk

Copies

SPECint_rate2006 = 40.8

SPECint_rate_base2006 = 36.9

0 88.0

3.00 7.00 11.0 15.0 19.0 23.0 27.0 31.0 35.0 39.0 43.0 47.0 51.0 55.0 59.0 63.0 67.0 71.0 75.0 79.0 83.0 8 47.6

8 72.8

8 20.9

4 26.6

8 29.9

8 35.8

4 38.9

8 57.2

8 65.4

8 39.7

8 46.3

8 49.3

8 44.5

8 81.7

8 87.6

8 14.7

8 17.8

8 23.8

4 23.8

8 44.4

Hardware

CPU Name: SPARC64 VII CPU Characteristics: CPU MHz: 2520 FPU: Integrated CPU(s) enabled: 4 cores, 1 chip, 4 cores/chip, 2 threads/core CPU(s) orderable: 1 chip Primary Cache: 64 KB I + 64 KB D on chip per core Secondary Cache: 5 MB I+D on chip per chip L3 Cache: None Other Cache: None Memory: 16 GB (2 GB x 8), 2-way interleaved Disk Subsystem: 73 GB 10,000 RPM Fujitsu MAY2073RC SAS Other Hardware: None

Software

Operating System: Solaris 10 10/08 Compiler: Sun Studio 12 with patches

124861-08, 124863-06, 124867-07, 127143-03, 127000-05, 127001-01 (see patch information below)

Auto Parallel: No File System: ufs System State: Default Base Pointers: 32-bit Peak Pointers: 32-bit Other Software: None

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org/

Page 2 spec^® SPEC CINT2006 Result

Copyright 2006-2014 Standard Performance Evaluation Corporation

Sun Microsystems Sun SPARC Enterprise M3000

SPECint_rate2006 = 40.8 SPECint_rate_base2006 = 36.9

CPU2006 license: 6 Test date: Sep-2008 Test sponsor: Sun Microsystems Hardware Availability: Oct-2008 Tested by: Fujitsu Limited Software Availability: Oct-2008

Results Table

Benchmark Copies Seconds Ratio Seconds Ratio Seconds Ratio

Base Copies Seconds Ratio Seconds Ratio Seconds Ratio

Peak

400.perlbench 8 1639 47.7 1643 47.6 1644 47.5 8 1079 72.4 1073 72.8 1073 72.8 401.bzip2 8 3701 20.9 3685 20.9 3701 20.9 4 1441 26.8 1450 26.6 1454 26.5 403.gcc 8 2155 29.9 2195 29.3 2129 30.2 8 2155 29.9 2195 29.3 2129 30.2 429.mcf 8 2036 35.8 2036 35.8 2036 35.8 4 938 38.9 939 38.9 940 38.8 445.gobmk 8 1467 57.2 1465 57.3 1475 56.9 8 1280 65.6 1286 65.2 1283 65.4 456.hmmer 8 1877 39.8 1879 39.7 1878 39.7 8 1877 39.8 1879 39.7 1878 39.7 458.sjeng 8 2092 46.3 2089 46.3 2090 46.3 8 1963 49.3 1963 49.3 1961 49.4 462.libquantum 8 3721 44.5 3723 44.5 3720 44.6 8 3721 44.5 3723 44.5 3720 44.6 464.h264ref 8 2168 81.7 2167 81.7 2156 82.1 8 2020 87.6 2015 87.9 2020 87.6 471.omnetpp 8 3409 14.7 3400 14.7 3406 14.7 8 2815 17.8 2816 17.8 2813 17.8 473.astar 8 2358 23.8 2359 23.8 2375 23.6 4 1181 23.8 1179 23.8 1172 24.0 483.xalancbmk 8 1240 44.5 1247 44.3 1243 44.4 8 1240 44.5 1247 44.3 1243 44.4

Results appear in the order in which they were run. Bold underlined text indicates a median measurement.

Compiler Invocation Notes

 Sun Studio compiler patches are available at
    http://developers.sun.com/sunstudio/downloads/patches/ss12_patches.jsp

Submit Notes

 The config file option ’submit’ was used.  Processes were assigned to
 specific processors using ’pbind’ commands.  The list of processors to use
 was provided in the ’BIND’ variable, to generate the pbind commands.
 (For details, please see the config file.)

Operating System Notes

 Shell Environments:
    Default setting.

 System Tunables:
 (/etc/system parameters)

    tune_t_fsflushr=10
       Controls how many seconds elapse between runs of the
       page flush daemon, fsflush.
    autoup=600
       Causes pages older than the listed number of seconds to
       be written by fsflush.
    bufhwm=3000
       Memory byte limit for caching I/O buffers.

Continued on next page

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org/

Page 3 spec^® SPEC CINT2006 Result

Copyright 2006-2014 Standard Performance Evaluation Corporation

Sun Microsystems Sun SPARC Enterprise M3000

SPECint_rate2006 = 40.8

SPECint_rate_base2006 = 36.9

CPU2006 license: 6 Test date: Sep-2008 Test sponsor: Sun Microsystems Hardware Availability: Oct-2008 Tested by: Fujitsu Limited Software Availability: Oct-2008

Operating System Notes (Continued)

    segmap_percent=1
       Set maximum percent memory for file system cache.

 Other System Settings:

    The webconsole service was turned off using svcadm disable webconsole.

Platform Notes

 Memory is 2-way interleaved by filling all slots with the same
 capacity DIMMs.

 This result is measured on a Fujitsu SPARC Enterprise M3000 Server.
 Note that the Fujitsu SPARC Enterprise M3000 and Sun SPARC Enterprise
 M3000 are electrically equivalent.

Base Compiler Invocation

C benchmarks:

cc

C++ benchmarks:

CC

Base Portability Flags

400.perlbench: -DSPEC_CPU_SOLARIS_SPARC

403.gcc: -DSPEC_CPU_SOLARIS 462.libquantum: -DSPEC_CPU_SOLARIS 483.xalancbmk: -DSPEC_CPU_SOLARIS

Base Optimization Flags

C benchmarks:

-fast -fma=fused -xipo=2 -xpagesize=4M -xprefetch_level=1
-xalias_level=std -ll2amm

C++ benchmarks:

-library=stlport4 -fast -fma=fused -xipo=2 -xpagesize=4M
-xprefetch_level=2 -xalias_level=compatible -lfast

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org/

Page 4 spec^® SPEC CINT2006 Result

Copyright 2006-2014 Standard Performance Evaluation Corporation

Sun Microsystems Sun SPARC Enterprise M3000

SPECint_rate2006 = 40.8

SPECint_rate_base2006 = 36.9

CPU2006 license: 6 Test date: Sep-2008 Test sponsor: Sun Microsystems Hardware Availability: Oct-2008 Tested by: Fujitsu Limited Software Availability: Oct-2008

Base Other Flags

C benchmarks:

-xjobs=4

C++ benchmarks:

-xjobs=4

Peak Compiler Invocation

C benchmarks:

cc

C++ benchmarks:

CC

Peak Portability Flags

400.perlbench: -DSPEC_CPU_SOLARIS_SPARC

403.gcc: -DSPEC_CPU_SOLARIS 462.libquantum: -DSPEC_CPU_SOLARIS 483.xalancbmk: -DSPEC_CPU_SOLARIS

Peak Optimization Flags

C benchmarks:

400.perlbench: -xprofile=collect:./feedback(pass 1)

-xprofile=use:./feedback(pass 2) -fast -fma=fused
-xpagesize=4M -xipo=2 -xalias_level=std -Xc -xrestrict
-lfast

401.bzip2: -xprofile=collect:./feedback(pass 1)

-xprofile=use:./feedback(pass 2) -fast -fma=fused
-xpagesize=4M -xalias_level=strong

403.gcc: basepeak = yes

429.mcf: -fast -fma=fused -xpagesize=4M -xipo=2 -xalias_level=std

-ll2amm

445.gobmk: -xprofile=collect:./feedback(pass 1)

-xprofile=use:./feedback(pass 2) -fast -fma=fused
-xpagesize=4M -xalias_level=std -xrestrict

Continued on next page

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org/

Page 5 spec^® SPEC CINT2006 Result

Copyright 2006-2014 Standard Performance Evaluation Corporation

Sun Microsystems Sun SPARC Enterprise M3000

SPECint_rate2006 = 40.8

SPECint_rate_base2006 = 36.9

CPU2006 license: 6 Test date: Sep-2008 Test sponsor: Sun Microsystems Hardware Availability: Oct-2008 Tested by: Fujitsu Limited Software Availability: Oct-2008

Peak Optimization Flags (Continued)

456.hmmer: basepeak = yes

458.sjeng: -xprofile=collect:./feedback(pass 1)

-xprofile=use:./feedback(pass 2) -fast -fma=fused
-xpagesize=4M -xipo=2

462.libquantum: basepeak = yes

464.h264ref: -xprofile=collect:./feedback(pass 1)

-xprofile=use:./feedback(pass 2) -fast -fma=fused
-xpagesize=4M -xipo=2 -xalias_level=std -m32
-xarch=sparcvis2 -xprefetch=no -ll2amm

C++ benchmarks:

471.omnetpp: -library=stlport4 -xprofile=collect:./feedback(pass 1)

-xprofile=use:./feedback(pass 2) -fast -fma=fused
-xpagesize=4M -xalias_level=compatible -xipo=2
-xprefetch_level=2 -Qoption cg -Qlp-av=0 -lfast

473.astar: -library=stlport4 -fast -fma=fused -xpagesize=4M

-xalias_level=compatible -xipo=2 -xprefetch_level=2 -lfast

483.xalancbmk: basepeak = yes

Peak Other Flags

C benchmarks:

-xjobs=4

C++ benchmarks:

-xjobs=4

The flags file that was used to format this result can be browsed at

http://www.spec.org/cpu2006/flags/Sun-Solaris-Studio12-and-gccfss4.2.r3.20090713.html

You can also download the XML flags source by saving the following link:

http://www.spec.org/cpu2006/flags/Sun-Solaris-Studio12-and-gccfss4.2.r3.20090713.xml

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org/

Page 6 spec^® SPEC CINT2006 Result

Copyright 2006-2014 Standard Performance Evaluation Corporation

Sun Microsystems Sun SPARC Enterprise M3000

SPECint_rate2006 = 40.8 SPECint_rate_base2006 = 36.9

CPU2006 license: 6 Test date: Sep-2008 Test sponsor: Sun Microsystems Hardware Availability: Oct-2008 Tested by: Fujitsu Limited Software Availability: Oct-2008

Originally published on 11 November 2008.

Report generated on Tue Jul 22 20:19:48 2014 by SPEC CPU2006 PS/PDF formatter v6932.

Tested with SPEC CPU2006 v1.1.

For other inquiries, please contact webmaster@spec.org.

For questions about this result, please contact the tester.

holders.

this result are trademarks or registered trademarks of their respective

Evaluation Corporation. All other brand and product names appearing in

SPEC and SPECint are registered trademarks of the Standard Performance